* + 1. Rim Mount Electric Strike:
       1. Product: 30-4-12 - Stainless steel electric strike designed for rim-type exit devices 12VDC@ 0.51Amp.
       2. Product: 30-4-24 - Stainless steel electric strike designed for rim-type exit devices 24VDC@ 0.25Amp.
       3. Finish: U - 630 Dull Stainless.

\*\* NOTE TO SPECIFIER \*\* Delete options not required.

* + - 1. Provide FS - Failsafe operation.
      2. Provide BR64XL - Rectifier.
      3. Provide LCBMA-30 - Latch and locking cam monitor.