* 1. STAND ALONE LOCKSETS
     1. Battery Powered Mortise Lockset with Digital Keypad, HID Compatible Prox Card/FOB Reader and Privacy Deadbolt
        1. Product: Model **E76+P** - EntryCheck Standalone Mortise Lockset with Digital Keypad, HID compatible Prox Card/FOB Reader and Privacy Deadbolt as manufactured by SDC Security Door Controls.
           1. Battery powered electronic mortise lockset for 3000 users. Standard features include an ANSI Grade 1 Mortise lockset with a lever clutch mechanism, 4-6 digit pin code, all weather keypad and housing, keypad or computer programming, 32 user groups, multi-year scheduling, temporary users, multiple zones, real time clock, auto daylight savings adjustment and more.
           2. Mortise lockset with 3/4 inch (19 mm) latch bolt with deadlatch. 4-7/8 inch (124 mm) strike standard.
           3. Door shall not unlock from outside keypad or Prox Reader operation when deadbolt is projected.
           4. Deadbolt shall be projected by inside thumb turn or outside key. Deadbolt retracted by inside thumb turn or outside key. Turning inside lever shall retract both the latch bolt and the deadbolt.
           5. HID compatible Proximity card and/or Proximity FOB reader
           6. UL Listed, USA and Canada for 3 hour "A" label fire rated doors. ANSI A156.25, Electrified Lockset Compliant. ANSI A156.13 Grade 1 Compliant.
           7. ANSI A117.1 Accessibility Code Compliant. ADA Compliant. California State Reference Code (Formerly Title 19, California State Fire Marshal): Compliant. Levers Galaxy, Eclipse and Nova return to within 1/2 inch (13mm) of the door face.

\*\* NOTE TO SPECIFIER \*\* Lever Handles with/without cylinders. Delete lever not required.

* + - 1. Handing: L - Left hand.
      2. Handing: LR - Left hand reverse
      3. Handing: R - Right hand.
      4. Handing: RR - Right hand reverse

\*\* NOTE TO SPECIFIER \*\* Black Dull Chrome is standard. Delete finish for keypad and lock that are not required.

* + - 1. Lever Trim: G - Galaxy with rose.
      2. Lever Trim: GE - Galaxy with escutcheon.
      3. Lever Trim: E - Eclipse with rose.
      4. Lever Trim: EE - Eclipse with escutcheon.
      5. Lever Trim: N - Nova with rose.
      6. Lever Trim: NE - Nova with escutcheon.
      7. Lever Trim: 07 - Schlage equivalent with SDC B rose.
      8. Lever Trim: 07E - Schlage equivalent with SDC escutcheon.
      9. Keypad Finish:

Q - Dull chrome

B – Black

* + - 1. Lock and Trim Finish:
         1. Q- Dull chrome
         2. C – Polished Brass
         3. P – Bright Chrome
      2. Keyed Cylinder Optional: CYL-6KDQ - 6 pin, 1.125 inches (29 mm) mortise cylinder, keyed different, dull chrome.
      3. Keyed Cylinder Optional: CYL-6KAQ - 6 pin, 1.125 inches (29 mm) mortise cylinder, keyed alike, dull chrome.
      4. Optional - Card: HID1326-100 ProxCard II (100 cards) as manufactured by SDC Security Door Controls.
      5. Optional - Card: HID1326-25 ProxCard II (25 cards) as manufactured by SDC Security Door Controls.
      6. Optional - Key Fob: HID1346-10 ProxKey II (10 key fobs) as manufactured by SDC Security Door Controls.
      7. Optional - Key Fob: HID1346-100 ProxKey II (100 key fobs) as manufactured by SDC Security Door Controls.